To flash the Etech-M Control Unit and Display

! your USB key must be formated in FAT32 
! your USB key size max 32GB

1. unzip the folder
2. copy all files from \Copy_To_USB to the root folder of your USB key
3. follow instruction from the manual


More information at : https://www.acv.com/international/page/usb-key-flash